todo(3)

NAME
todo - Todo List

Group avr_boot
    From email with Marek: On smaller devices (all except ATmega64/128), __SPM_REG is in the I/O space, accessible with the shorter 'in' and 'out' instructions - since the boot loader has a limited size, this could be an important optimization.